


PAVEMENT FORM 4 TRIAL 1 EXAMINATION 2022
Kenya Certificate of Secondary Education (K.C.S.E)
441/2
HOME SCIENCE
CLOTHING AND TEXTILES
PAPER 2
MARKING SCHEME
	NO.
	PROCESES 
	MAX. SCORE
	ACTUAL  SCORE
	REMARKS

	     
1.
	Presentation.
a) [bookmark: _GoBack]Work well pressed (1) and well folded (1).
b)   Label (½) firmly fixed (½) on a single fabric (½) without concealing details.( ½)
c)  Pins (1) and unnecessary tacking (1) removed from work. (1)
d) Making right half of skirt. (1)
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      2.
	
Cutting out.
a) All five pieces cut out. ( 5x½ )                             
b) Cutting of skirt front, skirt yoke, skirt back, waistband and 2 pocket sections on straight grain. (6x½)
c) Smooth cutting on CF of skirt front (½) and skirt yoke (½) and CB of skirt back (½). 
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   Back dart
a) Straight( ½) stitchery tapering to a point (½)
b) Dart secured at the point (½)
c) Correct length of the dart (10cm to within 2 mm. (½)
d) Correct width of dart.(accurate use of F.L) (½)
e) Dart pressed towards CB. (½)
f) Dart flat on R.S (½) and W.S (½)
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	4.


	     Inverted Pleat
a) Correctly made i.e must be inverted (1) 
b) Correctly held in yoke seam(1)
c) Good hang (1)
d) Accurate use of fold lines (2x½)
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	Overlaid seam (Yoke seam)
a) Folding of seam turning of skirt yoke along FL (½) onto the WS (½). 
b) Placing folded edge of yoke on RS (½) of skirt with fold matching FL (½).
c) Stitch from right side close to fold i.e 2mm from fold (½)
d)  Stitchery straight (½) correct tension (½ )
e)   Trimming (½) 10cm of seam turnings to 6mm (½) and neatening using loop stiches (1).Loop stitches: even (½) correct size(½)
f) Flat seam. (1)  
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	6.
	Inseam pockets.
a) Correct position (½),size (½) and shape (½).
b) Reinforced at the mouth i.e understitching of each pocket section. (2x1)
c) Trimming of seam turnings before under stitching. (2x½)
d) Inconspicuous on the RS. (1)
e) Flat (½)
f) Accurate use of FL when joining pocket sections to make pocket bag. (½)
g) Unneutered seam turnings of pocket bag.(½)
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	Side seam: Open neatened seam
(Award zero if not open seam)
a) Accurate use of FL. (1)
b)  Stitchery: correct size (½) correct tension(½) straight (½) 
c)  Correct width when finished – 1.2cm for    each turning. (2)
d)  Evenness in width (1)
e)  Well neatened (1) 
f) Seam pressed open (1) and flat at waistband (1) and hem (1) on both RS and WS.                     
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	8.
	      Waist band
a) Inner waistband interfaced (½).Interfacing firmly fixed. (½)
b) Accurate use of FL when attaching waistband.( ½)
c) Layering of seam turnings. (½)
d) Correctly positioned waistband i.e flash with CF of front skirt (½) and leave 4 cm overlap at the CB to within 3mm.( ½)
e) Fixing the waistband on W.S using even (½), correct size(½) of  hemming (½)stitches Hemming stitches slanting to the left.( ½) (Award zero if hemming stitches are not used) 
f) Good knife- edging  along the edge of the waistband (½) and well-made / sharp corners at the CB (on overlap) (½)
g) Flatness of the waistband on RS (½) and WS (½)
h) Evenness of the waistband (½) and correct finished width ( 3 cm) to within 3mm (½)
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